{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["48-h Mischprobe","Anleitung"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"48-h Mischprobe","index":0,"n_rows":22,"n_cols":16,"rows_kept":22,"cut":false,"hidden":false,"merged":[[8,4,8,5],[8,6,8,7],[9,4,9,5],[9,6,9,7],[10,4,10,5],[10,6,10,7],[12,4,12,5],[12,6,12,7],[13,4,13,5],[13,6,13,7],[11,6,11,7],[11,4,11,5]]}
[]
[]
[null,null,"Arbeitsblatt"]
[null,null,"Probenmischung 48-h-Mischprobe"]
[]
[null,null,"farbig hinterlegte Felder sind vom Kläranlagenpersonal auszufüllen"]
[]
[]
[null,null,null,null,"Tag 1",null,"Tag 2"]
[null,null,"Datum","[von - bis]*"]
[null,null,"Uhrzeit der Probenahme ","[von - bis]"]
[null,null,"Durchführende Person\nder Probenahme"]
[]
[null,null,"Abwassermenge während der\njeweiligen Probenahme","[m³]",null,null,null,null,null,null,null,{"$f":"IF(SUM(E14:H14)=0,\"\",SUM(E14:H14))","v":""}," m³",null,null,"Summe "]
[]
[]
[null,null,null,"%-Verhältnis",{"$f":"E14/L14*100","v":{"$error":"#VALUE!"}}," %",{"$f":"G14/L14*100","v":{"$error":"#VALUE!"}}," %"]
[]
[null,null,null,"erforderliches Volumen Zulauf",{"$f":"E17/100*L19*1000","v":{"$error":"#VALUE!"}}," mL",{"$f":"G17/100*L19*1000","v":{"$error":"#VALUE!"}}," mL",null,null,null,null," L",null,null,"Gesamtvolumen"]
[null,null,null,"erforderliches Volumen Ablauf",{"$f":"E17/100*L20*1000","v":{"$error":"#VALUE!"}}," mL",{"$f":"G17/100*L20*1000","v":{"$error":"#VALUE!"}}," mL",null,null,null,null," L",null,null,"Gesamtvolumen"]
[]
[null,null,"* bei Probenahmen, die nicht von 0:00 bis 0:00 Uhr durchgeführt werden, bitte den genauen Zeitraum angeben"]

{"sheet":"Anleitung","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}